jdott@stealth:~$ sudo btlejack -d /dev/ttyUSB0 -f 0xbc92f437

BtleJack version 2.0

[i] Using cached parameters (created on 2022-03-12 15:01:52)

[i] Detected sniffers:

> Sniffer #0: fw version 2.0

[i] Synchronizing with connection 0xbc92f437 ...

✓ CRCInit: 0xa06955

✓ Channel Map = 0x1fff3ffff8

✓ Hop interval = 168

✓ Hop increment = 6

[i] Synchronized, packet capture in progress ...

LL Data: 06 0f 0b 00 04 00 1b 12 00 00 00 00 00 01 00 00 00

LL Data: 0e 0b 07 00 04 00 52 12 00 00 00 01 01

LL Data: 06 1b 1a 00 04 00 1b 12 00 01 00 62 30 a4 01 ca 89 a9 5d 08 a4 d2 be e6 19 df 3a 2e d2

LL Data: 05 03 81 c3 74

LL Data: 1e 0b 07 00 04 00 52 12 00 00 00 01 00

LL Data: 02 0f 0b 00 04 00 52 12 00 00 00 00 00 01 00 2a a0

LL Data: 0a 0b 07 00 04 00 1b 12 00 00 00 01 01

LL Data: 02 1a 16 00 04 00 52 12 00 01 00 62 30 a4 01 ca 89 a9 55 04 a4 d2 b4 e0 11 c2 6c 21

LL Data: 0a 0b 07 00 04 00 1b 12 00 00 00 01 00